GT FIRMWARE UPGRADE INSTRUCTIONS

Note of Caution: Please confirm the correct version of firmware is downloaded and copied to the memory stick. There are 2 versions of firmware, one for the GT90 and one for the GT120.

1. Transfer the latest firmware image to the top folder of an external USB drive.
2. Power down the station with the rear panel switch.
3. Plug in the external drive to the USB port in the back of the station.



1. Press and hold “Menu” and “⮠ “ buttons simultaneously while switching the power button ON. Continue to hold “Menu” and “⮠ “ buttons the for 3 seconds then release them. The screen should remain dark for about 10 to 15 seconds. The unit will reset once the software is loaded successfully.

**NOTE: The display may show a high contrast. Once the EEPROM is reset and unit power cycled, the display will be reset properly.**

1. Verify the firmware version by observing the startup page. The model and version will be displayed for a few seconds before transitioning to the home status screen.
2. Clear the system memory settings **(Resetting the EEPROM)**
   1. Press and hold ▼▲ buttons simultaneously while switching the power button ON
   2. When the screen as shown below is displayed. Press, then release the “Menu” and “⮠ “ buttons simultaneously



1. Power cycle the unit as a final step to restore proper default settings. The software load is complete